**Work Instructions: How to clean out the Foam Generators**

**Parts Needed:**

* Foam Generator (P-CHE-2132): <https://shop.tommycarwash.com/Twist-n-Kleen-Foam-Generator-by-Mr-Foamer>
* Foam Generator Insert (P-CHE-2140): <https://shop.tommycarwash.com/Insert-for-Twist-and-Clean-Foam-Generator>

**Procedure:**

1. Disconnect the air line and detergent line from the foam generator.
2. Unscrew the foam generator from the Nozzle fitting.
3. Remove the cap of the Foam generator and remove the foam insert from the foam generator.
4. Rinse and clean any residue that is on the insert. Foam inserts with excess build-up can be soaked overnight in a 24:1 dilution ratio of Tommy Brite to water for extra cleaning.
5. Rinse and clean out the inside of the foam generator shell.
6. Reinsert the clean foam insert back into the clean foam generator shell and screw the cap back on.
7. Reinstall the newly cleaned foam generator back into its original position.
8. Reconnect the airline and detergent line to the Foam Generator.

**Instructional Video:**

[Foam Generator Clean Out on Vimeo](https://vimeo.com/553409699?embedded=true&source=vimeo_logo&owner=108168220)