**Work Instructions: How to clean out the Body Wax Manifold, Rain Bar, and Foamers**

**Potential Parts Needed:**

* C-Sprayer (P-M2086)
* Foam Generator (P-CHE-2132)
* Foam Generator Insert (P-CHE-2140)

**Tools Needed:**

* Tommy Brite or Dawn Dish Soap
* Power Sprayer
* Scotch-Brite Pad
* Ladder

**Procedure:**

1. Remove all three foamers from the manifold.
2. Take out the foam inserts and clean or replace them depending on the wear/age of the inserts.
3. Clean out the foam generators with Scotch-Brite pad, and Dawn Dish Soap, and rinse with the bay wash gun.
4. Remove the black foaming sprayers.
5. Spray out both sprayers with the bay wash gun.
6. Use the bay wash gun and spray out the wax manifold starting at one end. Repeat from the other end.
7. Spray each hole from underneath the manifold using the bash wash gun.
8. Reinstall all foamers and spray nozzles on the Body wax manifold.
9. Manually fire the Body Wax function to check correct coverage.
10. If you have holes on the manifold bar that are still clogged, you will need to reclean the Body Wax manifold bar.

**Instructional Video:**

[Body Wax Rain Bar Manifold on Vimeo](https://vimeo.com/552916089?embedded=true&source=vimeo_logo&owner=108168220)