Entrance-Exit Module Computer Maintenance

Frequency: Yearly

Action:

1. Blow out the junction box with canned air (Do not use an air hose as the oil can harm computer components).
2. Check to make sure all wires are secured and not wiggling loose.
3. Clean any corrosion. If there is any moisture, consider relocating/sealing the junction box.